Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a Fan Module

Note - This is a hot service procedure that can be performed by customers. See Hot Service, Replaceable by Customer for more information about hot service procedures.

The following procedure is based on the assumption that an empty slot exists for inserting the new fan module. If you need to remove a fan module before performing the installation procedure, see Remove a Fan Module.

1. Extend the server to the maintenance position.

   See Extend the Server.

2. Release the two fan compartment door latches and swing the door open.
3. Align the connector pins on the base of the new fan module with the connector on the fan module board and lower the module straight down into the slot.
4. Press down on the top of the module until it is fully seated.
5. Check the following status LEDs to verify that the new fan is functioning.

   - The fan module status LED associated with that fan module should be green. See Fan Module LEDs.

   - Both Service Required LEDs should be off.

6. Return the server to its operational position in the rack.

   SeeReturn the Server to the Normal Rack Position.

##### Related Information

- Fan Configuration Reference

- Fan Module LEDs

- Remove a Fan Module

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |