Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a SAS PCIe RAID HBA Card

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

| Caution - Components inside the chassis might be hot. Use caution when servicing components inside the chassis.

1. Unpack the SAS PCIe RAID HBA card and place it on an antistatic mat.
2. Remove the PCIe/XAUI riser that is closest to the power supplies.

   See Remove a PCIe or PCIe/XAUI Riser.

3. If a PCIe filler panel is installed, remove it.
4. Install the SAS PCIe RAID HBA card into the upper slot in the riser.

   Before inserting the card, you must rotate the retention clip out of the way, as shown in panel 1.

5. Rotate the retention clip downward and press it until it is securely in place.
6. Connect the internal data cables to the card.

##### Related Information

- Remove a SAS PCIe RAID HBA Card

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |