Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Supported DIMM Configurations

The following table describes supported memory configurations.

Note - All 1/4 and 1/2 configurations must have DIMM filler panels installed in all empty slots.

Table 27 Supported DIMM Configurations

DIMM Capacity | Number of DIMMs Installed | Total Memory Capacity
--- | --- | ---
4 GB | 4 (1/4 population) | 16 GB
| 8 (1/2 population) | 32 GB
| 16 (full population) | 64 GB
8 GB | 4 (1/4 population) | 32 GB
| 8 (1/2 population) | 64 GB
| 16 (full population) | 128 GB
16 GB | 4 (1/4 population) | 64 GB
| 8 (1/2 population) | 128 GB
| 16 (full population) | 256 GB
32 GB | 4 (1/4 population) | 128 GB
| 8 (1/2 population) | 256 GB
| 16 (full population) | 512 GB

##### Related Information

- DIMM Population Rules

- DIMM FRU Names

- DIMM Rank Classification Labels

- Increase System Memory With Additional DIMMs

- Verify DIMM Functionality

- DIMM Configuration Error Messages

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |