Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the DVD/USB Assembly

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Remove any optical disks from the DVD module and unplug any USB cables from the USB port.
3. Bring the server to the standby mode.

   Momentarily press the recessed Power button on the server front panel. You may need to use a pointed object, such as a stylus or pen.

4. Unplug the power cords.

   See Disconnect Power Cords .

5. Attach an antistatic wrist strap.
6. If the lower right hard drive bay contains an HDD or SDD module, remove it.

   This is the disk bay at location HDD7. See Hard Drive Slot Configuration Reference.

7. Reach in under the DVD/USB module and pull the release tab out.

   Use the finger indentation in the hard drive bay below the DVD/USB module to extend the release tab.

8. Slide the DVD/USB module out of the hard drive cage.
9. Place the module on an antistatic mat.

##### Related Information

- Install the DVD/USB Assembly

- DVD/USB Assembly Overview

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |