Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Secure Cables Using the CMA

Use the CMA to secure cables and ensure proper cable routing.

1. Remove the CMA cover.

   The CMA cover is secured with two No. 2 Phillips screws.

2. Place system cables into appropriate slots in the CMA.

   See Connecting the Server Cables.

3. Install the CMA cover.

   The cover is secured with two No. 2 Phillips screws.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |