Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Environmental Requirements

Specification | Operating | Nonoperating
--- | --- | ---
Temperature | Sea level to 2953 ft. (900m): 41`°`F to 95`°`F (5`°`C to 35`°`C) Above 2953 ft. (900m): Decrease the maximum allowable temperature by 1.6`°`F/1000 ft (1`°`C/300m) IEC 60068-2-1 Test Ad, and 60068-2-2 Test Bd | -40`°`F to 149`°`F (-40`°`C to 65`°`C) IEC 60068-2-1 Test Ab and 60068-2-2 Test Bb
Relative Humidity | 10 to 90% RH, 27`°`C maximum wet bulb (noncondensing) IEC 60068-2-56 Test Cb | 93% RH, 35`°`C maximum wet bulb (noncondensing) IEC 60068-2-56 Test Cb
Altitude | 10,000 ft. (3,000m)1 IEC 60068-2-13 Test M, and 60068-2-41 Test Z/BM | 40,000 ft. (12,000m) IEC 60068-2-13 Test M
Vibration | 0.15 G (z-axis), 0.10 G (x-, y-axes), 5-500Hz swept sine IEC 60068-2-6 Test Fc | 0.5 G (z-axis), 0.25 G (x-, y-axes), 5-500Hz swept sine IEC 60068-2-6 Test Fc
Shock | 3 Gs, 11 ms half-sine IEC 60068-2-27 Test Ea | Roll-off: 1-inch roll-off free fall, front to back rolling directions Threshold: 25 mm threshold height at 0.75 m/s impact velocity ETE-1010-02 Rev A

1Except in China markets where regulations may limit installations to a maximum altitude of 2000 m.

##### Related Information

- Physical Specifications

- Input Power Information

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |