Skip Navigation Links
Exit Print View
| SPARC T4-4 Server ### Product Notes

Search Scope:

- This Document
- Entire Library

## Support for 1.5 TByte Memory Configuration

The SPARC T4-4 server supports a 1.5 TByte memory configuration.

Note - The 1.5 TByte configuration requires system firmware no earlier than 8.3.0.b.

For specific DIMM installation and configuration instructions, see the SPARC T4-4 Server Service Manual.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |