Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Rack Compatibility

The rackmount kit is compatible with equipment racks that meet the following standards:

- Four-post structure (mounting at both front and rear).

  Note - Two-post racks are not compatible.

- Rack horizontal opening and unit vertical pitch conforming to ANSI/EIA 310-D‐1992 or IEC 60927 standards.

- Distance between front and rear mounting planes between 24 to 36 inches (65 cm and 91.5 cm).

- Minimum clearance depth (to front cabinet door) in front of front rackmount plane: 1 inch (25.4 mm).

- Minimum clearance depth (to rear cabinet door) behind front rackmount plane: 34.6 inches (88 cm) with cable management assembly (recommended) or 31.5 inches (80 cm) without the cable management assembly.

- Minimum clearance width (between structural supports and cable troughs) between front and rear mounting planes: 18.9 inches (48 cm).

##### Related Information

- Tools Needed for Installation

- Rackmount Kit

- Determine Correct Rackmount Hardware

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |