Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Hot Spare Drives in RAID Volumes (LSI)

You can configure two global hot spare drives to protect data on mirrored RAID volumes. If one of the drives in a RAID 1 or RAID 1E mirrored volume fails, the onboard RAID controller will replace the failed drive automatically with a hot spare drive and then resynchronize the mirrored data.

Use the `sas2ircu` LSI utility to add global hot spare drives or HMP. Refer to the SAS2 Integrated RAID Solution User Guide for more information about adding hot spare drives.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |