Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a Hard Drive

1. Align the replacement drive to the drive slot and slide the drive in until it is seated.

   Drives are physically addressed according to the slot in which they are installed. If you are replacing a drive, install the replacement drive in the same slot as the drive that was removed. See Hard Drive Configuration Reference for drive slot information.

2. Close the latch to lock the drive in place.
3. Verify the drive functionality.

   See Verify Hard Drive Functionality.

##### Related Information

- Hard Drive Hot-Pluggable Capabilities

- Hard Drive Configuration Reference

- Hard Drive LEDs

- Locate a Faulty Hard Drive

- Remove a Hard Drive

- Verify Hard Drive Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |