Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

###### Single-Processor Module Configurations

In single-processor module configurations, the processor module must be installed in PM Slot 0. A PM filler panel must be installed in PM Slot 1.

Note - All DIMMs installed in the server must have identical capacities. In addition, all DIMMs related to each CMP must have identical architectures. For more information, see DIMM Population Rules (Except 1536-Gbyte Configurations) and DIMM Rank Classification.

Table 19 Supported Memory Configurations (Single Processor Module Configurations)

Total Amount of Memory | Processor Module 0 | Processor Module 1
--- | --- | ---
64 Gbytes | Half-Populated Processor Module 4-Gbyte DIMMs in CMP 1 group 4-Gbyte DIMMs in CMP 0 group | Processor filler module
128 Gbytes | Fully-Populated Processor Module (Except 1536 Gbyte Configurations) 4-Gbyte DIMMs in CMP 1 group 4-Gbyte DIMMs in CMP 0 group | Processor filler module
128 Gbytes | Half-Populated Processor Module 8-Gbyte DIMMs in CMP 1 group 8-Gbyte DIMMs in CMP 0 group | Processor filler module
256 Gbytes | Fully-Populated Processor Module (Except 1536 Gbyte Configurations) 8-Gbyte DIMMs in CMP 1 group 8-Gbyte DIMMs in CMP 0 group | Processor filler module
256 Gbytes | Half-Populated Processor Module 16-Gbyte DIMMs in CMP 1 group 16-Gbyte DIMMs in CMP 0 group | Processor filler module
512 Gbytes | Fully-Populated Processor Module (Except 1536 Gbyte Configurations) 16-Gbyte DIMMs in CMP 1 group 16-Gbyte DIMMs in CMP 0 group | Processor filler module
512 Gbytes | Half-Populated Processor Module 32-Gbyte DIMMs in CMP 1 group 32-Gbyte DIMMs in CMP 0 group | Processor filler module
1024 Gbytes | Fully-Populated Processor Module (Except 1536 Gbyte Configurations) 32-Gbyte DIMMs in CMP 1 group 32-Gbyte DIMMs in CMP 0 group | Processor filler module

##### Related Information

- Servicing Processor Modules

- DIMM Population Rules (Except 1536-Gbyte Configurations)

- Half-Populated Processor Module

- Fully-Populated Processor Module (Except 1536 Gbyte Configurations)

- Dual-Processor Module Configurations

- DIMM Rank Classification

- Install a DIMM

- Increase Memory With Additional DIMMs

- Verify DIMM Functionality

- Understanding DIMM Configuration Error Messages

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |