Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

###### Fully-Populated Processor Module (1536-Gbyte Configuration)

Note - 1536-Gbyte configurations require System Firmware 8.3.0.b or later.

The DIMM slots are color-coded to help you determine how the slots should be populated. In a 1536-Gbyte configuration, each processor module is populated as follows:

- Blue color-coded DIMM slots: Populated with 32-Gbyte 4Rx4 DIMMs

- White color-coded DIMM slots: Populated with 32-Gbyte 4Rx4 DIMMs

- Black color-coded DIMM slots: Populated with 16-Gbyte 2Rx4 DIMMs

Note - To determine DIMM rank classification, see DIMM Rank Classification.

The following figure shows how the DIMMs are installed in a 1536-Gbyte configuration.

Table 18 Legend for 1536-Gbyte Configuration

Symbol | Meaning
--- | ---
| Denotes a slot populated with a 32-Gbyte 4Rx4 DIMM.
| Denotes a slot populated with a 16-Gbyte 2Rx4 DIMM.

##### Related Information

- DIMM Population Rules (Except 1536-Gbyte Configurations)

- Fully-Populated Processor Module (Except 1536 Gbyte Configurations)

- Single-Processor Module Configurations

- Dual-Processor Module Configurations

- DIMM Rank Classification

- Install a DIMM

- Increase Memory With Additional DIMMs

- Verify DIMM Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |