Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Gigabit-Ethernet Ports

Four RJ-45 Gigabit Ethernet connectors (NET0, NET1, NET2, NET3) are located on the system back panel. The Ethernet interfaces operate at 10 Mbit/sec, 100 Mbit/sec, and 1000 Mbit/sec.

Pin | Signal Description | Pin | Signal Description
--- | --- | --- | ---
1 | Transmit/Receive Data 0 + | 5 | Transmit/Receive Data 2 –
2 | Transmit/Receive Data 0 – | 6 | Transmit/Receive Data 1 –
3 | Transmit/Receive Data 1 + | 7 | Transmit/Receive Data 3 +
4 | Transmit/Receive Data 2 + | 8 | Transmit/Receive Data 3 –

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |