Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the CMA

The CMA is attached to the center rear of the server.

Note - The CMA installation might block some of the power outlets in the cabinet, making them unavailable.

1. Install the L brackets at the rear . The brackets are marked “Left” and “Right” as viewed from the back of the server.

   Repeat for left and right sides:

   1. Identify the “left” and “right” side brackets.
   2. Remove the two middle screws from the rackmount adaptor.
   3. Place the bracket over the center two mounting holes.
   4. Secure each mounting bracket with two No. 2 Phillips screws.
2. Slide the left and right swivel clips into the left and right L brackets.
3. Secure the CMA with the two captive screws.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |