Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the Ethernet Network Cables

The server has four network connectors, marked NET0, NET1, NET2, and NET3. These connectors are RJ-45 Gigabit Ethernet. See Rear Panel Components for connector locations.

Note - The ILOM sideband management feature enables you to access the SP using one of these Ethernet ports. Refer to the SPARC T3 Series Servers Administration Guide for instructions.

1. Connect a Category 5 (or better) cable from your network switch or hub to Ethernet Port 0 (NET0) on the rear of the chassis.
2. Connect Category 5 (or better) cables from your network switch or hub to the remaining Ethernet ports (NET1, NET2, NET3), as needed.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |