Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the NET MGT Cable

- Connect a Category 5 cable from the service processor network management port to your network switch or hub. See Rear Panel Components for connector locations.

  The service processor network management port is labeled NET MGT. This port is not operational until you configure the network settings (through the serial management port), as detailed in Log In to the SP (SER MGT Port).

  If you have access to a DHCP server on the network, you can see the service processor get an IP address because the DHCP client is enabled by default.

  Note - The NET MGT port is configured by default to retrieve network settings with DHCP and allow connections using SSH. You might need to modify these settings for your network. Instructions are given in Powering On the Server for the First Time.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |