Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Mapping WWN Values to Hard Drives (OBP `probe-scsi-all` Command)

These topics explain how to map WWN values to specific SAS2 drives using the OBP command `probe-scsi-all`. Separate explanations are provided for each SPARC T4-x server model.

- `probe-scsi-all` WWN Mapping Overview

- `probe-scsi-all` WWN Mapping Example (SPARC T4-1)

- `probe-scsi-all` WWN Mapping Example (Netra SPARC T4-1)

- `probe-scsi-all` WWN Mapping Example (SPARC T4-2)

- `probe-scsi-all` WWN Mapping Example (Netra SPARC T4-2)

- `probe-scsi-all` WWN Mapping Example (SPARC T4-4 With Four CPUs)

- `probe-scsi-all` WWN Mapping Example (SPARC T4-4 With Two CPUs)

- `probe-scsi-all` WWN Mapping Example (SPARC T4-1B and Netra SPARC T4-1B)

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |