Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Locate a Faulty Service Processor Card

Before You Begin

The following LEDs are lit when a SP fault is detected:

- System Service Required LEDs on the front panel and rear I/O module

- Server SP Status LED on the main module or rear I/O module

1. Determine if the System Service Required LEDs are lit on the front panel or the rear I/O module.

   See Interpreting Diagnostic LEDs.

2. Check the SP Status LED on the main module or the rear I/O module to determine if the service processor card needs to be replaced.

   See Main Module Motherboard LEDs or Rear I/O Module LEDs. The SP Status LED will be lit amber if the service processor needs to be replaced.

3. Remove the faulty service processor card.

   See Remove the Service Processor Card.

##### Related Information

- Service Processor Card Overview

- Remove the Service Processor Card

- Install the Service Processor Card

- Verify Service Processor Card Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |