Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect a Terminal or Emulator to the SER MGT Port

- Connect a terminal or a terminal emulator (PC or workstation) to the service processor serial management port.

  Configure the terminal or terminal emulator with these settings:

  - 9600 baud
  - 8 bits
  - No parity
  - 1 Stop bit
  - No handshake

  A null modem configuration is needed, meaning the transmit and receive signals are reversed (crossed over) for DTE to DTE communications. You can use the supplied RJ-45 crossover adapters with a standard RJ-45 cable to achieve the null modem configuration.

  Note - When you power on the server for the first time and you do not have a terminal or terminal emulator (PC or workstation) connected to the service processor serial management port, you will not see system messages.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |