Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Input Power Information

The maximum operating input current values are based on the formula P / (V *0.90), where P = maximum operating input power and V=input voltage. For example: 620W / (100V * 0.90) = 6.89A. You can use this formula to calculate the maximum operating current at your input voltage.

##### Related Information

- Electrical Specifications‘

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |