Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Understanding DIMM Configurations

These topics provide the information that you will need to determine how many DIMMs to install in the processor modules, where those DIMMs should be installed on the processor modules, and what size DIMM you should use.

Description | Links
--- | ---
Understand the DIMM population rules. | DIMM Population Rules (Except 1536-Gbyte Configurations) DIMM Population Rules (1536-Gbyte Configuration)
Understand the different DIMM configuration options that are available to you. | Half-Populated Processor Module Fully-Populated Processor Module (Except 1536 Gbyte Configurations)
Determine how to populate the DIMM slots in the processor modules depending on the following factors: The number of processor modules in your server The capacity of the DIMMs that you have available The total amount of memory that you would like in each processor module | Single-Processor Module Configurations Dual-Processor Module Configurations
Understand the concept of DIMM architecture, as defined by the DIMM classification label. | DIMM Rank Classification

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |