Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### FRU Paths (2 Running Processor Modules)

This express module topology is for a server with two running processor modules installed.

In this scenario, the FRU path for express module slot 7 (EM7) follows this path, starting from the processor module:

1. Processor 2 in processor module 1, to

2. PCIe switch 0, to

3. Express module slot 7 (EM7)

In this scenario, the full FRU path for EM7 is:

`/pci@600/pci@2/pci@0/pci@0`

Note that the final `pci@` path in the full FRU path changes from `pci@6` in a single-processor module scenario to `pci@0` for a dual-processor module scenario (see FRU Paths (1 Running Processor Module) for the full FRU path for EM7 in a single-processor module scenario). Express module slot 7 is the only express module slot where the final `pci@` path in the full FRU path would change between a single-processor module scenario and a dual-processor module scenario.

As a second example, the FRU path for express module slot 8 (EM8) will follow this path, starting from the processor module:

1. Processor 1 in processor module 0, to

2. PCIe switch 1, to

3. Express module slot 8 (EM8)

In this scenario, the full FRU path for EM8 is:

`/pci@500/pci@1/pci@0/pci@1`

##### Related Information

- FRU Paths (1 Running Processor Module)

- FRU Paths (1 Failed Processor Module)

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |