Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Assigning a Static IP Address to the SP

If your network does not use DHCP, the network management port is not operational until you configure network settings for the service processor.

This topic includes the following tasks:

- Oracle ILOM System Console Overview

- Log In to the SP (SER MGT Port)

- Assign a Static IP Address to the NET MGT Port

##### Related Information

- Oracle ILOM System Console Overview

- Oracle Solaris OS Configuration Parameters

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |