Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

###### Half-Populated Processor Module

A half-populated processor module has the following characteristics:

- Eight 4, 8, 16, or 32-Gbyte DIMMs installed in the slots related to CMP 1

- Eight 4, 8, 16, or 32-Gbyte DIMMs installed in the slots related to CMP 0

The DIMM slots are color-coded to help you determine which slots should be populated for different configurations. In a half-populated configuration, the slots are populated as follows:

- Blue color-coded DIMM slots: Populated

- White color-coded DIMM slots: Populated

- Black color-coded DIMM slots: Populated with DIMM filler panels

The following figure shows how the DIMMs are installed in a half-populated processor module configuration.

Table 16 Legend for Half-Populated PM

Symbol | Meaning
--- | ---
| Denotes a populated slot.
| Denotes a slot populated with a DIMM filler panel.

##### Related Information

- DIMM Population Rules (Except 1536-Gbyte Configurations)

- Fully-Populated Processor Module (Except 1536 Gbyte Configurations)

- Single-Processor Module Configurations

- Dual-Processor Module Configurations

- DIMM Rank Classification

- Install a DIMM

- Increase Memory With Additional DIMMs

- Verify DIMM Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |