Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Server

| Caution - A fully configured server weighs 175 lbs (80 kg). Use a mechanical lift to install the server into the rack.

1. Ensure the mechanical lift is level and stable.
2. Lift the server up to the correct height.
3. Slide the server into the rack.

   Ensure that the bottom edge of the server has cleared the bottom of the rack rails.

   Figure 6 Installing the Server

   Figure Legend

   1 Mechanical lift

   2 SPARC T4-4 server

   3 Cabinet

   4 Shelf rail

   5 Ensure server mounted above shelf rail

4. Secure the server to the front panel using four No. 2 Phillips screws.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |