Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### DIMM Configuration Errors (`fmadm faulty` Output)

The fault management tool (`fmadm`) captures DIMM configuration errors. For example:

    faultmgmtsp> fmadm faulty
    ------------------- ------------------------------------ -------------- ------
    Time                UUID                                 msgid          SeverityFRU         : /SYS/PM0/CMP0/BOB0/CH0/D0              (Part Number: 000-0000)              (Serial Number: 00CE011217213B151F)Description : A FRU has been inserted into a location where it is not              supported.Response    : The service required LED on the chassis may be illuminated.Impact      : The FRU will not be usable in its current location.Action      : The administrator should review the ILOM event log for              additional information pertaining to this diagnosis.  Please              refer to the Details section of the Knowledge Article for              additional information.
    ------------------- ------------------------------------ -------------- ------
    2012-09-24/17:00:40 2caf416b-4fe0-6509-db02-aa719f5dd543 SPT-8000-PX    Major

    Fault class : fault.component.misconfigured

##### Related Information

- DIMM Configuration Errors (System Console)

- DIMM Configuration Errors (`show faulty` Command Output)

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |