Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### SER MGT Ports

The SER MGT port is an RJ-45 connector. There is one SER MGT port on the the back panel. This port is the default connection to the system console.

An additional SER MGT port is located on the main module, and is accessible from the front panel.

Table 1 Serial Management Connector Signals

Pin | Signal Description | Pin | Signal Description
--- | --- | --- | ---
1 | Request to Send | 5 | Ground
2 | Data Terminal Ready | 6 | Receive Data
3 | Transmit Data | 7 | Data Set Ready
4 | Ground | 8 | Clear to Send

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |