Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### DIMM Population Rules (1536-Gbyte Configuration)

The following population rules apply to 1536-Gbyte configurations:

- There are 32 DDR3 DIMM slots on each processor module.

- On each processor module, 16 DIMM slots (four banks, with four DIMM slots in each bank) are associated with CMP0. The other 16 DIMM slots (four banks, with four DIMM slots in each bank) are associated with CMP1. The figures in the following topics show which DIMM slots are associated with which CMP.

- Any DIMM slot that does not have a DIMM installed must be populated with a DIMM filler.

- DIMMs must be installed as described in Fully-Populated Processor Module (1536-Gbyte Configuration).

Note - 2Rx4 16-Gbyte DIMMs and all 32-Gbyte DIMMs require System Firmware 8.2.1.b at minimum. See DIMM Rank Classification.

Note - The 1536-Gbyte configuration requires System Firmware 8.3.0.b at minimum.

##### Related Information

- Half-Populated Processor Module

- Fully-Populated Processor Module (Except 1536 Gbyte Configurations)

- Fully-Populated Processor Module (1536-Gbyte Configuration)

- Single-Processor Module Configurations

- Dual-Processor Module Configurations

- Remove a DIMM

- Install a DIMM

- Verify DIMM Functionality

- Increase Memory With Additional DIMMs

- Increase Memory With Additional DIMMs (16-Gbyte Configurations)

- DIMM Rank Classification

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |