Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the SER MGT Cable

The service processor serial management port is marked SER MGT. See Front Panel Components and Rear Panel Components for connector locations.

- Connect a Category 5 cable from the service processor SER MGT port to the terminal device.

  Use this port for initial server management. This port is needed to activate the NET MGT port, as detailed in Powering On the Server for the First Time.

  When connecting either a DB-9 or a DB-25 cable, use an adapter to perform the crossovers given for each connector.

  Note - Use the service processor serial management port only for server management. It is the default connection between the service processor and a terminal or a computer.

  | Caution - Do not attach a modem to the service processor serial management port.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |