Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Front I/O Assembly

| Caution - This procedure requires that you handle components that are sensitive to static discharge. Static discharges can cause the components to fail.

1. Take the necessary ESD precautions.

   See Prevent ESD Damage.

2. Insert the front I/O assembly into position in the main module.

   - Gently slide the front I/O assembly into position with the ports inserted into the port holes in the front of the main module.

   - Lower the rear of the front I/O assembly so that the captive screw is aligned with the screw hole on the motherboard.

3. Tighten the captive screw to secure the front I/O assembly to the motherboard.
4. Connect the two cables.
   1. Lower into place the connectors that secure the FIO-to-motherboard cable to the front I/O assembly and the motherboard and press down on both connectors to connect the FIO-to-motherboard cable.
   2. Lower into place the connectors that secure the VGA-to-motherboard cable to the front I/O assembly and the motherboard and press down on both connectors to connect the VGA-to-motherboard cable.
5. Install the main module back into the server.

   See Install the Main Module.

##### Related Information

- Front I/O Assembly Overview

- Remove the Front I/O Assembly

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |