Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Rear I/O Module

1. Take the necessary ESD precautions.

   See Prevent ESD Damage.

2. With the lever in the lowered position, insert the rear I/O module into the slot at the rear of the server.
3. Raise the extraction lever up until it clicks into place, fully seating the rear I/O module into the server.
4. Connect the cables to the appropriate ports on the rear I/O module.
5. Power on the server.

   See Returning the Server to Operation.

6. Verify the rear I/O module functionality.

   See Verify Rear I/O Module Functionality.

##### Related Information

- Rear I/O Module LEDs

- Locate a Faulty Rear I/O Module

- Remove the Rear I/O Module

- Verify Rear I/O Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |