Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### QSFP Port

The QSFP connector is a 10-Gigabit XUAI port connection.

Pin | Signal | Pin | Signal | Pin | Signal | Pin | Signal
--- | --- | --- | --- | --- | --- | --- | ---
1 | GND | 11 | SCL | 21 | RX2n | 31 | Reserved
2 | TX2n | 12 | SDA | 22 | RX2p | 32 | GND
3 | TX2p | 13 | GND | 23 | GND | 33 | TX3p
4 | GND | 14 | RX3p | 24 | RX4n | 34 | TX3n
5 | TX4n | 15 | RX3n | 25 | RX4p | 35 | GND
6 | TX4p | 16 | GND | 26 | GND | 36 | TX1p
7 | GND | 17 | RX1p | 27 | ModPrsL | 37 | TX1n
8 | ModSeIL | 18 | RX1n | 28 | IntL | 38 | GND
9 | LPMode_Reset | 19 | GND | 29 | VccTx |  |
10 | VccRx | 20 | GND | 30 | Vcc1 |  |

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |