Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## R

  rackmounting, Installing the Server

  racks, compatible, Rack Compatibility

  RAID
    configuring, Configuring Hardware RAID
    creating volumes, Create a Hardware RAID Volume
    `FCode`utility, Prepare to Use the FCode Utility
    support, Hardware RAID Support

  RAID expansion modules
    FRU name, FRU Reference
    installing, Install the RAID Expansion Module
    locating, Main Module Components
    removing, Remove the RAID Expansion Module

  rear chassis subassembly
    installing, Install the Rear Chassis Subassembly
    locating, Rear Panel Components
    overview, Rear Chassis Subassembly Overview
    removing, Remove the Rear Chassis Subassembly

  rear components, Rear Panel Components

  Rear Express Module Fault LED, Interpreting Diagnostic LEDs

  Rear Fan Module Fault LED, Interpreting Diagnostic LEDs

  rear I/O module
    FRU name, FRU Reference
    installing, Install the Rear I/O Module
    LEDs, Interpreting Diagnostic LEDs
    locating, Rear Panel Components
    removing, Remove the Rear I/O Module
    verifying functionality, Verify Rear I/O Module Functionality

  removing
    DIMMs, Remove a DIMM
    express modules, Remove an Express Module
    fan modules, Remove a Fan Module
    front I/O assembly, Remove the Front I/O Assembly
    hard drives, Remove a Hard Drive
    main module, Remove the Main Module
    main module motherboard, Remove the Main Module Motherboard
    power supplies, Remove a Power Supply
    processor modules, Remove a Processor Module
    RAID expansion modules, Remove the RAID Expansion Module
    rear chassis subassembly, Remove the Rear Chassis Subassembly
    rear I/O module, Remove the Rear I/O Module
    service processor, Remove the Service Processor Card
    storage backplanes, Remove a Storage Backplane
    system battery, Remove the System Battery
    system configuration PROM, Remove the System Configuration PROM

  reset, resetting the system with`uadmin`, Reset the Server

  restart behavior
    setting the boot timeout interval, Set the Boot Timeout Interval
    specifying behavior at boot timeout, Specify Behavior at Boot Timeout
    specifying behavior if restart fails, Specify Behavior if Restart Fails
    specifying behavior when host stops running, Specify Behavior When the Host Stops Running
    specifying max restart attempts, Specify Maximum Restart Attempts
    specifying on host reset, Specify Behavior When the Host Resets

  RJ-45 cable, Cabling Requirements

  running POST in Diag Mode, Run POST With Maximum Testing

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |