Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Prevent ESD Damage

Many components housed within the chassis can be damaged by ESD. To protect these components from damage, perform the following steps before opening the chassis for service.

1. Prepare an antistatic surface to set parts on during the removal, installation, or replacement process.

   Place ESD-sensitive components, such as the printed circuit boards, on an antistatic mat. The following items can be used as an antistatic mat:

   - Antistatic bag used to wrap a replacement part
   - ESD mat
   - A disposable ESD mat (shipped with some replacement parts or optional server components)
2. Attach an antistatic wrist strap.

   When servicing or removing server components, attach an antistatic strap to your wrist and then to a metal area on the chassis.

##### Related Information

- Safety Information

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |