Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Rackmount Hardware

1. Repeat the following steps for both the left and right front mounting points:
   1. Place the adaptor bracket in the marked location.

      Note - An “up” arrow indicates proper orientation.

   2. Secure the adaptor bracket, with one No. 2 Phillips screw in the center hole.
   3. Insert a mounting clip in the hole just above the top of the rack rail bracket.
2. Repeat the following steps for both the left and right rear mounting points:
   1. Place the adaptor bracket in the marked location.

      Note - An “up” arrow indicates proper orientation.

   2. Secure the adaptor bracket top and bottom holes, with two No. 2 Phillips screws.
3. Install the left and right upper corner brackets.
   1. Install two cage nuts into the cabinet in the two holes above the tops of the adaptor brackets.
   2. Secure each upper curner bracket with two No. 2 Phillips screws.
4. Install the shelf rails.

   Note - The shelf rails are marked “Left” and “Right” (as viewed from the front of the server) and “Front” and “Rear.”

   Repeat for left and right shelf rails:

   1. Insert the front of the shelf rail into the front adaptor bracket.
   2. Insert the rear of the shelf rail into the rear adaptor bracket.

      The shelf rail slides in and out to fit cabinets of different depths.

   3. Secure each shelf rail with two flat-head No. 2 Phillips screws.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |