Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Locate a Faulty Hard Drive

Before You Begin

The following LEDs are lit when a hard drive fault is detected:

- System Service Required LEDs on the front panel and rear I/O module

- Service Required LED on the faulty drive

1. Determine if the System Service Required LEDs are lit on the front panel or the rear I/O module.

   See Interpreting Diagnostic LEDs.

2. From the front of the server, check the drive LEDs to identify which drive needs to be replaced.

   See Hard Drive LEDs. The amber Service Required LED will be lit on the drive that needs to be replaced.

3. Remove the faulty drive.

   See Remove a Hard Drive.

##### Related Information

- Hard Drive Hot-Pluggable Capabilities

- Hard Drive Configuration Reference

- Hard Drive LEDs

- Remove a Hard Drive

- Install a Hard Drive

- Verify Hard Drive Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |