# Insert WS-Addressing

## Contents
Overview Configuration

## Overview
The WS-Addressing specification defines a transport-independent standard for including addressing information in SOAP messages. The Enterprise Gateway can generate WS-Addressing information based on a configured endpoint in a policy, and then insert this information into SOAP messages.
## Configuration
Complete the following fields to configure the Enterprise Gateway to insert WS-Addressing information into the SOAP message header. Name: Enter an appropriate name for the filter. To: The message is delivered to the specified destination. From: Informs the destination server where the message originated from. Reply To: Indicates to the destination server where it should send response messages to. Fault To: Indicates to the destination server where it should send fault messages to. MessageID: A unique identifier to distinguish this message from others at the destination server. It also provides a mechanism for correlating a specific request with its corresponding response message. Action: The specified action indicates what action the destination server should take on the message. Typically, the value of the WS-Addressing `Action` element corresponds to the SOAPAction on the request message. For this reason, this field defaults to the `soap.request.action` message attribute. Relates To: If responses are to be received asynchronously, the specified value provides a method to associate an incoming reply to its corresponding request. Namespace: The WS-Addressing namespace to use in the WS-Addressing block.