2.2. Features
Prev | Chapter 2. Sun Ray 3 Client | Next

## 2.2. Features

The following table summarizes the main features of the Sun Ray 3 Client.

Table 2.1. Sun Ray 3 Client Features

Feature | Details
--- | ---
Ethernet Port | 10/100/1000 Megabit per second (RJ45)
Serial Port | Single 16550 compatible serial port (DB9)
USB | Five USB 2.0 compliant ports, one on front panel, four on rear panel
Video Graphics Resolutions | Support for graphics resolutions of up to 1920x1200 via a single-link DVI-I video connector.
Audio | Stereo headphone output jack (1/8" mini-jack) Microphone input jack (1/8" mini-jack) Internal 2 Watt monaural speaker
Power Status LED | Off/Green/Amber (Off/On/Fault)
ON/OFF Switch | Capacitance-sensing, soft-touch Power ON/OFF switch
Smart Card Reader | Lighted Smart Card slot indicates Smart Card access activities Supports ISO 7816 T=0 and T=1 interface smart cards (synchronous cards not supported) Dual-sided reader socket Supported card voltages: 1.8V, 3V, 5V Maximum card baud rate: 230 K
System Security Lock | Security Lock Slot
ENERGY STAR Compliance | Version 5.0, Category A
MTBF | 200,000 hours minimum at 25C (calculated)

Prev | Up | Next
2.1. Part Numbers | Home | 2.3. Ports