4.9. MTBF, Reliability, and Other Standards
Prev | Chapter 4. Sun Ray 3i Client | Next

## 4.9. MTBF, Reliability, and Other Standards

The calculated mean time between failures is 75,000 hours minimum at 25C. Compliance with reliability and other standards is documented in the following table.

Table 4.4. Sun Ray 3i Client Reliability and Other Standards

IEC 60068-1 | Environmental Testing - Part 1: General and guidance
IEC 60068-2-1 | Environmental Testing - Part 2: Tests A: Cold -50
IEC 60068-2-2 | Environmental Testing - Part 2: Tests B: Dry heat +140
IEC 60068-2-3 | Environmental Testing - Part 2: Test Ca: Damp heat
IEC 60068-2-6 | Environmental Testing - Part 2: Test Fc and guidance: Vibration (sinusoidal)
IEC 60068-2-13 | Environmental Testing - Part 2: Test M: Low air pressure
IEC 60068-2-27 | Environmental Testing - Part 2: Test Ea and guidance: Shock
IEC 60068-2-31 | Environmental Testing - Part 2: Test Ec: Drop and topple, primarily for equipment-type specimens
IEC 60068-2-32 | Environmental Testing - Part 2: Test Ed: Free fall
IEC 60068-2-56 | Environmental Testing - Part 2: Test Cb: Damp heat, steady state, primarily for equipment
IEC 60068-2-64 | Environmental Testing - Part 2: Test Fh: Vibration, broad-band random (digital control) and guidance
ASTM D3332 | Standard Test Methods for Mechanical-Shock Fragility of Products, Using Shock Machines
U.S. CFR1194 | Section 508 of the U.S. Rehabilitation Act of 1986, as amended by the Workforce Investment Act of 1998

Prev | Up | Next
4.8. Power Supply | Home | 4.10. Operating Conditions