3.5. Graphics
Prev | Chapter 3. Sun Ray 3 Plus Client | Next

## 3.5. Graphics

A high-performance graphics chip provides high-resolution graphics on dual analog or digital displays, using Dual-Link DVI-I connectors, with the following resolutions and timings for each port:

- 640x480x60

- 640x480x75

- 640x480x85

- 800x600x60

- 800x600x75

- 800x600x85

- 1024x768x60

- 1024x768x75

- 1024x768x85

- 1152x900x66

- 1152x900x76

- 1280x800x60

- 1280x1024x60

- 1280x1024x66

- 1280x1024x75

- 1280x1024x76

- 1280x1024x85

- 1400x1050x60

- 1440x900x60

- 1600x1024x60

- 1600x1200x60

- 1600x1200x75

- 1680x1050x60

- 1920x1080x60

- 1920x1080x70

- 1920x1080x72

- 1920x1200x60

- 1920x1200x70

- 2560x1600x60

Note

The maximum display resolution is 2560x1600 at 24 bits per pixel.

Although the Sun Ray 3 Plus Client can produce both analog (HD15) and digital video (DVI) output, a DVI cable is always recommended to ensure the best performance and should be used whenever possible.

Prev | Up | Next
3.4. Chassis | Home | 3.6. Network Interfaces