4.10. Operating Conditions
Prev | Chapter 4. Sun Ray 3i Client | Next

## 4.10. Operating Conditions

The Sun Ray 3i Client operates within the ranges specified in the following tables.

Table 4.5. Sun Ray 3i Client Operating Conditions

Temperature | 0 to 40C
Humidity | 5% to 93% RH
Altitude | 3 km (9,842 feet)
Acoustic Noise Emissions | Less than 30dBA for any case, at 0.25m from the case in any direction per ISO 9296, 7779, and 9295

Table 4.6. Sun Ray 3i Client Non-Operating Conditions

Temperature | -20 to 60C
Humidity | 5% to 93% RH
Altitude | 12 km (39,370 feet)

Prev | Up | Next
4.9. MTBF, Reliability, and Other Standards | Home | 4.11. LED Indicators