2.4. Chassis
Prev | Chapter 2. Sun Ray 3 Client | Next

## 2.4. Chassis

The Sun Ray 3 Client enclosure provides passive cooling and can be used in a vertical position, supported by its base. There are no user accessible items or moving parts.

Table 2.2. Sun Ray 3 Client Mechanical Dimensions

Dimension | Detail
--- | ---
Width | 28 mm (1.10 in.)
Depth | 158 mm (6.22 in.)
Height (without base) | 190 mm (7.48 in.)
Height (with base) | 196 mm (7.72 in.)
Weight (without base) | 500 g (1.10 lb.)
Weight (with base) | 660 g (1.46 lb.)

Prev | Up | Next
2.3. Ports | Home | 2.5. Graphics