4.4. Chassis
Prev | Chapter 4. Sun Ray 3i Client | Next

## 4.4. Chassis

The Sun Ray 3i Client enclosure provides passive cooling and can be used in portrait orientation, supported by its base or mounted to the wall using the VESA-compliant mount feature located on the rear of the enclosure. There are no user accessible items or moving parts.

Table 4.2. Sun Ray 3i Client Mechanical Dimensions

Dimension | Detail
--- | ---
Width | 517.40 mm (20.37 in.)
Depth (with rear cover) | 48.50 mm (1.91 in.)
Height (without base) | 308.80 mm (12.16 in.)
Height (with base) | 407.90 mm (16.06 in.)
Weight (without base and rear cover) | 4.22 kg (9.30 lb.)
Weight (with base) | 5.45 kg (12.02 lb.)

Prev | Up | Next
4.3. Ports | Home | 4.5. Flat Panel Display