4.2. Features
Prev | Chapter 4. Sun Ray 3i Client | Next

## 4.2. Features

The following table summarizes the main features of the Sun Ray 3i Client.

Table 4.1. Sun Ray Client 3i Features

Feature | Details
--- | ---
Ethernet Port | 10/100/1000 Megabit per second (RJ45)
Serial Port | Single 16550 compatible serial port (DB9)
USB | Five USB 2.0 compliant ports, two on the left side of the front panel, one on the left rear panel, and two on the center rear panel.
Integrated Flat Panel Display | 21.5-inch color AM-TFT-LCD Display format (fixed resolution): 1920x1080 pixels Contrast ratio: 1000:1 (typical) Luminance: 250 cd/m2 (typical) Response time: 5.0 ms (total response time, typical) Horizontal viewing angle: ± 85 degrees (for CR>10) (typical) Vertical viewing angle: ± 80 degrees (for CR>10) (typical) 2-lamp cold cathode fluorescent lamp backlight
Base | Tilt adjustment and manual swivel only
Analog Video Out | Supports a fixed graphics resolution of 1920x1080@60Hz via an HD-15 (VGA) analog video port
Audio | Stereo headphone output jack (1/8" mini-jack) Microphone input jack (1/8" mini-jack) Internal 2 Watt monaural speaker
Power Status LED | Off/Green/Amber (Off/On/Fault)
ON/OFF Switch | Capacitance-sensing, soft-touch Power ON/OFF switch
Brightness Control | Luminance intensity (brightness) control switch
Smart Card Reader | Lighted Smart Card slot indicates Smart Card access activities Supports ISO 7816 T=0 and T=1 interface smart cards (synchronous cards not supported) Dual-sided reader socket Supported card voltages: 1.8V, 3V, 5V Maximum card baud rate: 230 K
System Security Lock | Security lock slot
ENERGY STAR Compliance | Version 5.0, Category A
MTBF | 75,000 hours minimum at 25C (calculated)

Prev | Up | Next
4.1. Part Numbers | Home | 4.3. Ports