Skip Headers

StorageTek SL3000 Systems Assurance Guide E20876-08 |
| Contents

Previous |

# Index

A B C D E F G H I L M N O P R S T V W

## Numerics

  2N, 5.1.2
  2N+1, 5.1.2

## A

  Access Expansion Module, 2.1.5
  access plates, fire suppression locations, 7.3
  ACSLS, 3.3.1
  active capacity, 4.2
  AEM, 2.1.5
  AEM specifications, 7.1.4
  Airborne Contaminants, 7.5.3
  arbitrated loop, 3.1.1.1
  arrays
    tape drives
      performance zone, A.2.3.6
      planning for optimization, A.1.6, A.2.3.2
  automated cartridge system library software, 3.3.1

## B

  bar-code
    camera, Glossary
    scanner, 2.2.2, 3.1
  base module
    installation time estimate, 8.3
    installation tool kit, 8.6.3
    specifications
      shipping, 8.4, 8.4
  Btu per hour, Glossary
  Btu/hr, 5.5
  bulk loading, 2.1.5

## C

  cable routing, 7.4
  cables
    AC power, 5.4
    Ethernet, 9.9.2
    fiber-optic part numbers/lengths, 9.9
  camera, bar-code, Glossary
  CAP
    drive expansion module, 2.1.2.1
    enter/eject cartridges, A.2.1
    optimizing, A.2.1
  CAP Labels, A.1.5
  capacity
    active, 4.2
    capcity on demand, 4.2
    examples, 4.1.1
    physical, 4.1
    real time growth, 4.2
  Capacity on Demand, described, A.2.3.2
  CAPs
    bulk load capabilities, A.1.3
  cartridge
    optimization, A.2.1
  cartridge access port, A.2.1
  cartridge expansion module
    installation time estimates, 8.3, 8.3, 8.3
    specifications
      shipping, 8.4, 8.4
  cartridges
    float option, A.2.1
    optimization, A.2.1
  CDRT, 3.3.2.3
  cells
    capacities, 4.2
  changes to document, Preface
  CLI, 2.2.1.1
  client system component, 3.4.5
  clustering
    cartridges, A.2.1
    drives, A.1.6
  CO2 emissions, 5.5
  command line interface, 2.2.1.1
  components
    software, 1.2
      library management applications, 3.3
      StorageTek Library Console, 3.2.1
  concurrent disaster recovery test, 3.3.2.3
  configurations
    AC power options, 5.1.1
  conformance, standards, D
  connections
    Fibre Channel (library), 2.2.1, 3.1.1
    TCP/IP, 2.2.1, 3.1.2
  connector types
    TCP/IP, 3.1.2
  contaminants, 7.5.3
  content management
    cartridges, A.2.1
    drives, A.2.1
    media, A.2.1
    philosophy, A.2
    tape cartridges, A.2.1
    tape drives, A.1.6
  cooling, 5.6
  CSC, 3.4.5
  customer
    AC power requirements, 5.1.1
    floor requirements, 8.1
  cutouts, floor, 7.4

## D

  DC power
    configurations, 5.2
  dimensions
    base module
      shipping, 8.4, 8.4
    cartridge expansion module
      shipping, 8.4
    drive expansion module
      installed, 2.1.2.1
      shipping, 8.4
    parking expansion module
      shipping, 8.4
  distribution pads, 7.2.1.1
  drive expansion module
    installation time estimates, 8.3
    installation tool kit, 8.6.3
    specifications
      installed, 2.1.2.1
      shipping, 8.4, 8.4
  dual
    TCP/IP
      connections, 3.1.2
  Dual TCP/IP
    description, 3.1.2.1
  dynamic World Wide Name, A.4.1

## E

  earthquakes, 7.5.2
  ECM
    power, 5.2.2
  eject operations
    CAP optimization, A.2.1
    cartridges, A.2.1
  electromagnetic, compatibility standards, D
  ELS, 3.3.2, Glossary
  Encryption Capable Tape Drives, B.2
  enter operations
    CAP optimization, A.2.1
    cartridges, A.2.1
  enterprise library software, 3.3.2
  Ethernet
    cables, 9.9.2
  expert performance reporter, 3.4.4
  Extended High Performance Data Mover, 3.4.6
  extractor tool, used for power rail, 8.6

## F

  FC-SCSI, 3.1.1
  features, 1.1
  fiber-optic cables
    part numbers/lengths, 9.9
  Fibre Channel
    arbitrated loop, 3.1.1.1
    cables, 9.9
    switched fabric, 3.1.1.1
    topology, 3.1.1.1
  fire suppression
    access plates, 7.3
    planning, 7.3
  fire suppression planning, 7.3
  fire suppression, access plates, 7.3
  float, option used for optimization, A.2.1
  floor
    customer, installation requirements, 8.1
    weight capacity, 7.2.1
  floor cutouts, 7.4

## G

  gaseous limits, 7.5.3

## H

  hardware
    tools required for installation, 8.6
  hardware activation files, 4.2
  host software component, 3.3.2.1
  HSC, 3.3.2.1

## I

  independent software vendors, 3.3.3
  installation
    AC power cables, 5.4
    fiber-optic cables, 9.9
    personnel required, 8.3
    time estimates, 8.3, 8.3, 8.3
    tools
      base module kit, 8.6.3
      drive expansion module kit, 8.6.3
      required, 8.6, 8.6
  interfaces
    Fibre Channel
      library, 3.1.2
      tape drive data side, 9.9.1
    TCP/IP
      protocol, 3.1.2
  ISVs, 3.3.3

## L

  labels
    cartridges, ordering, 9.7
  labels, CAP, A.1.5
  LCM, 3.4.3
  library
    system assurance, Preface, 6
  Library Console, 3.2.1
  library content manager, 3.4.3
  library features, 1.1
  library management software
    ACSLS, 3.3.1
    CDRT, 3.3.2.3
    ELS, 3.3.2
    HSC, 3.3.2.1
    SMC, 3.3.2.1
    VTCS, 3.3.2.2
  library size, 4.1
  LINKLIBs, 3.3.2.1
  Log SnapShot feature, 3.2.3

## M

  media optimization, A.2.1
  minimum
    working area, 8.1
  monitoring, 3.2

## N

  N+1, 5.1.2
  network
    SNMP application, 3.2.2
  network configuration, A.3

## O

  optimization guidelines
    cartridges, A.2.1
    media, A.2.1
    planning, A.2
    tape cartridges, A.2.1
    tape drives, A.1.6
  options
    AC power configurations, 5.1.1
  ordering, 9
    cables
      Fibre Channel, 9.9.1
    cartridge labels, 9.7
    cartridges, 9.7

## P

  parking expansion module
    dimensions
      shipping, 8.4
  part numbers
    AC power cables, 5.4
    cable
      Fibre Channel, 9.9.1
    cables
      Ethernet, 9.9.2
      Fibre Channel, 9.9.1
    installation tools, 8.6
    tool kit, 8.6
  partitioning
    described, A.2.3.2
    rectangular boundaries, A.2.3.2
  performance zone
    described, A.2.3.6
  philosophy for content management, A.2
  physical capacity
    calculating, 4.1
    examples, 4.1.1
  planning
    checklist, 7
  power
    AC
      cables, 5.4
      configurations, 5.1.1, 5.1.1
      options, 5.1.1
      redundant, 5.1.2
    cable routing, 7.4
    DC
      cPCI supplies, 5.2
      load sharing supplies, 5.2
    requirements, 5.1.1
    T9840 power-up tool, 8.6.1
  power consumption, 5.5
    calculation, 5.5.1
  power rail
    extractor tool, 8.6
    TallBot operation, 2.2.2
  power redundancy options, 5.1.2
  power supplies
    ECM, 5.2.2
    robotics, 5.2.1
    tape drives, 5.2.3, 5.3
  pre-installation planning
    checklist, 7
  process, for system assurance, Preface, 6

## R

  rail
    power enable modules required, 5.2
  rectangular boundaries, partitioning, A.2.3.2
  redundant
    AC power, 5.1.2
  redundant robotics feature
    AEM, 2.1.5.1
  Redundent Electronics (RE), 2.2.1.2
  robotics
    power, 5.2.1

## S

  safety
    fire suppression access plates, 7.3
  scratch
    cartridge optimization, A.2.1
  seismic compatibility, 7.5.2
  shipping
    module specifications, 8.4, 8.4
    pallets
      specifications, 8.4
  SL Console, 3.2.1
  SLC, 3.2.1
  slot capacity, 4.1
  slots
    capacities, 4.2
  SMC, 3.3.2.1
  SNMP
    library support, 3.2.2
  software
    independent vendors, 3.3.3
    library management applications, 1.2, 3.3
    SNMP protocol supported, 3.2.2
    StorageTek Library Console, 3.2.1
  specifications
    drive expansion module, 2.1.2.1
    shipping, 8.4, 8.4
  STA, 3.4.7
  Standards of Conformance, D, D
  storage capacity, 4.1
  storage management component, 3.3.2.1
  StorageTek Library Console, 3.2.1
    described, 3.2.1
  StorageTek Tape Analytics, 3.4.7
  summary of changes, Preface
  Switched Fabric, 3.1.1.1
  switched fabric, Fibre Channel topology, 3.1.1.1
  system assurance
    process overview, Preface, 6

## T

  T10000
    description, B.1.1, B.1.2
  T9840
    description, B.1.1
    power-up tool, 8.6.1
  TallBot
    DC power supplies required, 5.2
    illustrated, 2.2.2, 3.1
    redundant (dual)
      illustrated, 2.2.2, 3.1
  tape cartridge content management, A.2.1
  tape drive comparison, B.1.5
  tape drives
    content management, A.1.6
    DC power supplies required, 5.2
    dynamic World-Wide Name, A.4.1
    power, 5.2.3
    power supply calculation, 5.3
    supported types, B.1.4
    T10000, B.1.2
      described, B.1.1
    T9840, B.1.1
      power-up tool, 8.6.1
  TCP/IP
    connection, 3.1.2
    connections, 2.2.1, 3.1.2
    interfaces supported, 3.1.2
    protocol, 3.1.2
  tools
    required for installation, 8.6
    T9840 tape drives, drive power-up, 8.6.1
  topology
    switched fabric, 3.1.1.1
  T-Series
    T10000, B.1.2
    T9840, B.1.1

## V

  virtual library extension, 3.4.2.1
  virtual private network, A.3
  virtual storage manager, 3.4.2
  virtual tape, 3.4.2
  Virtual Tape Control System, 3.3.2.2
  VLE, 3.4.2.1
  VPN, A.3
  VSM, 3.4.2
  VTCS, 3.3.2.2

## W

  weight
    distribuiton pads, 7.2.1.1
    floor capacity, 7.2.1, 8.1
  working area, 8.1