Skip Headers

StorageTek SL3000 User's Guide E20875-05 |
| Contents

Previous |

# Index

A B C D E F G H I K L M N O P R S T U V W

## A

  access door
    closing, 13.4.2
    opening, 13.4.1
    safety interlocks, 13.2.1
    safety release, 13.2.3
  activated capacity
    active storage regions, 4.1
      defining, 4.3.1
      reports, 4.3.2
    cell activation rules, 4.1
    changes and FC-SCSI connections, 4.1.2
    changes and HLI connections, 4.1.1
    orphaned cartridges and, 4.1.3
  activated features
    display current, 3.6
    install, 3.2
  active storage regions
    automatic assignment, 4.1
    defining, 4.3.1
    manual assignment, 4.1
    reports, 4.3.2
  addressing, A
    AEMs internal firmware, A.7.1.2
    CAPs HLI, A.7.2
    CAPs internal firmware, A.7.1
    FC-SCSI, A.4
    HLI-PRC, A.3
    internal firmware, A.2
    tape drives, A.6
  AEM
    allocating to partitions, 5.1
    associating to a partition, 5.8.1
    emergency access, 13.4.3
    library partitions and, 5.1
    properties, 8.4.1
    rebooting, 11.1.1
    removing partition associations, 5.8.1
    status, 8.4.1
    summary information, 8.4.1
    using to bulk load cartridges, 8.3
    using to bulk unload cartridges, 8.3
  AEM access door
    audits and, 13.4.4
    closing, 8.5
    fast access, 13.4.3
  AEM operations
    summarized, 8.3
  AEM safety door
    properties, 8.4.2
    status, 8.4.2
  audits
    audit indicator, 6.11
    description, 6.11
    full library, 6.11.1.1
    main access door and, 6.11
    physical, 6.11.1, 6.11.1.1, 6.11.1.2
    range of cells, 6.11.1.2
    verified, 6.11.2
  auto enter mode (CAPs)
    described, 8.1
  automated mode
    returning the library to, 6.9.3

## B

  barcode presentation, 10.2.1, 10.2.1

## C

  CAP associations
    library partitions and, 5.3.2, 5.8.1
    removing, 5.8.1
  CAP reservations
    library partitions and, 5.2.2
    overriding, 5.8.2
  capacity
    activated. See activated capacity.
  CAPs
    and library partitions, 5.1
    auto enter mode, 8.1
    closing, 8.5
    display properties, 8.4.1
    display status, 8.4.1
    display summary information, 8.4.1
    inserting cartridges, 10.7
    library partitions and, 5.1, 5.8
    making available for diagnostic moves, 8.6
    manual mode, 8.1
    self-test, 8.7, 9.6
    states
      library partitions and, 5.2.2.2, 5.3.2.1, 8.1.1
    varying offline, 8.8
    varying online, 8.8
  cartridges
    applying labels, 10.10.4
    barcode presentation, 10.2.1, 10.2.1
    display information, 10.4
    ejecting into a partition, 5.8.1
    ejects, 10.8
    entering into a partition, 5.8.1
    enters, 10.7
    exterior cleaning, 10.10.2
    handling, 10.10
    inserting in a cell or drive, 10.10.1
    inserting in the CAP, 10.7
    inspecting, 10.10.1
    list, 10.4
    loading through the AEM, 8.3
    locate by address, 10.5.2
    locate by VOLID, 10.5.1
    locating by address, 10.5
    locating by VOLID, 10.5
    move by VOLID, 10.6.1
    move from specified location, 10.6.1
    recovery moves, 10.6
    storing, 10.10.3
    unlabeled, 10.2
    unloading through the AEM, 8.3
  cautions
    reentering cleaning cartridge, 10.1
    solvents for cleaning a cartridge, 10.10.2
  CenterLine, A.1
  cleaning cartridges, 10.1
    exporting, 9.1.7.2
    importing, 9.1.7
    list, 9.1.4
    warning threshold, 9.1.6

## D

  device status, 6.1
    listing codes, 12.6
  diagnostic cartridges
    description, 10.9
    exporting, 10.9.2
    importing, 10.9.1
    library self-tests and, 6.7
    management tasks, 10.9
  diagnostic moves (robot)
    controlling, 11.6.5
    defining, 11.6.1
    description, 11.6
    managing definitions, 11.6.2
    monitoring, 11.6.5
    pool address range, 11.6
    random access order, 11.6
    robot selection, 11.6
    saving, 11.6.3
    sequential access order, 11.6
    starting, 11.6.4
    target address range, 11.6
  diagnostic support files, 12.2
  diagnostics
    CAPs and, 8.6
  domain, media labels, 10.2
  drive cleaning
    configuring library auto clean, 9.1.5
    description, 9.1
    display status of, 9.2
    exporting cleaning cartridges, 9.1.7.2
    importing cleaning cartridges, 9.1.7
    library auto clean, 9.1.2
    manual, 9.1.3
  drive controller, 6.4.2
  Drive Events Report, 9.3
  Drive Media Events Report, 9.3
  drive trays
    status, 9.2
  drive VOP
    displaying for T10000, 9.2
  drives
    bringing online, 9.5
    cleaning. See drive cleaning.
    display drive properties, 9.2
    display drive summary information, 9.2
    display status, 9.2
    LED status, 9.2
    network data, 9.2
    SCSI FastLoad and, 11.2.1.1, 11.2.1.1
    states, 9.5
    taking offline, 9.5

## E

  eject operations, 10.8
    partitioned libraries, 5.8.1
  enter operations, 10.7
    partitioned libraries, 5.8.1
  event monitors
    description, 12.4.1
    display, 12.5.1
    display multiple, 12.5.3
    spool data to a file, 12.5.2

## F

  FC-SCSI elements, A.4
  FC-SCSI interface, 6.10
    barcode presentation and, 10.2.1, 10.2.1
    FastLoad feature and, 11.2.1.1, 11.2.1.1

## G

  General Events Statistics Report, 6.4.3.3, 6.4.3.3

## H

  hardware activation file
    comparing to current features, 3.4
    delete, 3.5
    description, 3.1
    display current, 3.6
    displaying contents of, 3.4
    download, 3.3
    Feature Audit Log, 3.7
    file type, 3.1
    install, 3.4
    installing, 3.2
  hardware activation key file
    overlaying, 3.1.1
  hardware activation tasks, 3.2
  HLI interface, 6.10
    displaying port status, 6.4.1
  HLI-PRC addressing, A.3
  host interfaces
    changing the type, 6.10
    HLI. See HLI interface., 6.4.1
    non-partitioned libraries and, 6.10

## I

  internal firmware addressing, A.2

## K

  key
    maintenance, 13.1

## L

  library
    placing in manual mode, 6.9.1
    placing online, 6.9.2
    returning to automated mode, 6.9.3
  library auto clean, 9.1.2
  library configuration
    display, 6.4.2
  library controller
    display redundant electronics, 7.4, 7.4
    log in to alternate, 7.2.3
    properties, 6.4.2
  library events, 12.4
  library events. See Also event monitors.
  library firmware upgrades, 6.2
    activate, 6.2.2
    download, 6.2.1
  library initialization sequence, 13.3.2
  library partitions
    AEM associations and, 5.8.1
    allocating an AEM CAP, 5.1
    barcode presentation and, 10.2.1
    CAP associations and, 5.3.2, 5.8.1, 5.8.1
    CAP reservations and, 5.2.2, 5.8.2
    CAP states and, 5.2.2.2, 5.3.2.1, 8.1.1
    commit configuration changes, 5.7.4
    configuration tasks, 5.7
    create, 5.7.2
    delete, 5.7.2.2
    described, 5
    design, 5.7.3
    displaying, 4.3.3, 5.7.6
    ejecting cartridges into, 5.8.1
    entering cartridges into, 5.8.1
    hosts and, 5
    library hardware changes and, 5.5
    library resources and, 5.6
    orphaned cartridges in, 10.3
    reports, 5.7.5
    SCSI FastLoad feature and, 11.2.1.1
    shared CAPs and, 5.3.2
    using AEMs in, 5.1
    using CAPs in, 5.1
    using CAPs with, 5.1
    verify, 5.7.3
  library power down, 13.3.1
  library power up, 13.3.2
  library reboot, 6.8
  library reports, 2.5
    displaying, 6.4.3
    saving data to a file,SL Console report tasks, 6.4.3
    searching, 6.4.3
  library self-tests, 6.7, 12.1
    performing, 6.7, 6.7
  library status, 6.1
    display, 6.4.1
  local operator panel
    described, 2.9
    entering data, 2.9.1
    factory alignment, 2.9.3
    logging in, 2.9.2
    re-calibrating, 2.9.3
    virtual keypad, 2.9.1
  log snapshot file
    generating process, 6.5.2
    transfer process, 6.5.2
  login IDs, 2.6.1
  logs
    Feature Audit Log, 3.7

## M

  main access door
    audits and, 6.11
  maintenance key, 13.1
  manual CAP, 8.1
  manual cleaning (drive), 9.1.3
  manual mode
    placing the library in manual mode, 6.9.1
    returning the library to automated mode, 6.9.3
  manual operations
    safety precautions, 13.2
      access door interlocks, 13.2.1
      access door release, 13.2.3
      general, 13.2
      server power interrupt, 13.2.2
  media
    domain labels, 10.2
    ID labels, 10.2
  MIB file
    described, 12.2
    transfer process, 6.5.1

## N

  non-disruptive partitioning
    FC-SCSI partitions and, 5.3.1
    HLI partitions and, 5.2.1

## O

  orphaned cartridges
    non-partitioned libraries and, 4.1.3
    partitioned libraries and, 10.3

## P

  Pass-thru Ports (PTPs)
    locating cartridges, 10.5
  passwords
    activation, 2.6.2
    modifying, 2.6.2.1
  placing the library in manual mode, 6.9.1
  port bonding, 6.4.1
  ports
    status, 6.4.1
  power down the library, 13.3.1
  power supplies
    monitoring tasks, 6.4.4
    status of, 6.4.4
    summary information, 6.4.4
  power up the library, 13.3.2

## R

  reboot
    library, 6.8
  recovery moves, 10.6
  redundant electronics
    manual switch, 7.5
    tasks, 7.4
  reports
    cartridge summary, 10.4
    cartridge table, 10.4
    drive events, 9.3
    feature audit log, 3.7
  result codes
    listing, 12.6
  returning the library to automated mode, 6.9.3
  robot
    display status of, 11.3
    display summary information, 11.3
    monitoring tasks, 11.3
    properties, 11.3
    SCSI FastLoad and, 11.2.1.1, 11.2.1.1
    self-test, 11.5
    varying offline, 11.4
    varying online, 11.4

## S

  safety precautions, 13.2
    access door interlocks, 13.2.1
    access door release, 13.2.3
    general, 13.2
    servo power interrupt, 13.2.2
  SCSI FastLoad, 11.2.1.1, 11.2.1.1
  self-tests
    CAP, 8.7
    drive, 9.6
    library, 6.7, 6.7, 6.7, 12.1
    robot, 11.5
  SL Console
    activation password, 2.6.2, 2.6.2
    communications failures, 6.1
    description, 2
    first-time access, 2.6.2
    logging off, 2.6.4
    login ID, 2.6.1
    modes, 2.1
    modifying passwords, 2.6.2.1
    screen, components, 2.3
    screen, modifying layout, 2.3.1
    security, 2.6
    synchronize with library, 2.3.2.1
    user ID, 2.6.1
  SL Console Help
    description, 2.4
    navigation, 2.4
  SL Console reports
    Drive Events, 9.3
    Drive Media Events, 9.3
    General Events, 6.4.3.3, 6.4.3.3
    types, 2.5.1
  SLConsole
    downloading, 2.2
    media pack, 2.2
  SNMP
    transfer the library MIB file, 6.5.1
  standalone SL Console
    description, 2.8
    logging in, 2.8.4
  standalone SLConsole
    updating, 2.8
  status
    library and devices, 6.1
  status alerts
    clearing, 6.6
    described, 6.4.1
    displaying, 6.4.1

## T

  tape drives
    addressing, A.6
    hardware numbering, A.6.1
    HLI-PRCs, A.6.3
    internal firmware address, A.6.2
  transferring the log snapshot file, 6.5.2
  troubleshooting, 12.3

## U

  User ID
    types, 2.6.1

## V

  vary the library offline, 6.9.1
  vary the library online, 6.9.2
  VOP
    displaying for T10000 drives, 9.2

## W

  Web-launched SL Console
    client requirements, 2.7.2
    description, 2.7
    logging in using a browser, 2.7.3
    logging in using an icon, 2.7.4
    logging in using CLI, 2.7.3
    security, 2.7.1
    starting on a client, 2.7.3
    updating on a client, 2.7
  web-launched SLConsole
    installing, 2.7