Skip Headers

StorageTek SL150/SL500/SL3000/SL8500 SNMP Reference Guide E35317-03 |
| Contents

Previous |

# Index

A C D F H L M N P R S T V

## A

  access control, 2.2.4
  agent
    embedded SNMP, 3.1
    trap
      slAgentTest, 3.3.2
      slAgentTestHeartbeatA, 3.3.3
      slAgentTestHeartbeatB, 3.3.4
      slTrapAgentStart, 3.3.1
    variables, 1.3

## C

  CAP, 1.4
  cell, 1.5
  controller, 1.7

## D

  drive, 1.8.1

## F

  fan, 1.10
  FRU variables
    slControllerFru, 1.7
    slTrapAsrSuspectCount, 1.19.1
    slTrapAsrSuspectFruChassisId, 1.19.1
    slTrapAsrSuspectFruManufacturer, 1.19.1
    slTrapAsrSuspectFruName, 1.19.1
    slTrapAsrSuspectFruPn, 1.19.1
    slTrapAsrSuspectFruRevision, 1.19.1
    slTrapAsrSuspectFruSn, 1.19.1
    slTrapAsrSuspectFruStatus, 1.19.1
    slTrapAsrSuspectIndex, 1.19.1
    slTrapConfigDeviceId, 1.19.2
    slTrapDeviceId, 1.19
    slTrapSvcDeviceEventOpCode, 1.19.3

## H

  hardware
    CAP, 1.4
    cell, 1.5
    controller card, 1.7
    drive, 1.8
    elevator, 1.9, 1.9
    environment or condition, 3.3.7
    fan, 1.10
    media event, 1.8.3
    power supply, 1.14.1
    PTP, 1.13
    redundant power, 1.14.2
    robot, 1.15
    safety door, 1.16
    tape, 1.18
    turntable, 1.20
  host interface, 1.11

## L

  library
    cleaning, 1.6
    condition, 1.12.1
    configuration, 1.12.2
    date, 1.12.3
    identifying information, 1.12.4
    location, 1.12.5
    network, 1.12.6
    state, 1.12.7
    statistics, 1.12.8
    temperature, 1.12.9
    version, 1.12.10

## M

  Management Information Base. See MIB
  media event, 1.8.3
  MIB
    definition, 1
    obtaining, 2.5.1

## N

  network, 1.12.6

## P

  partition variables
    slCellPartition, 1.5
    slCellPartitionType, 1.5
    slTapePartition, 1.18
    slTapePartitionType, 1.18
  port
    disable portID, 2.8.2
    enable portID, 2.8.1
  port variables
    slAgentPort, 1.3
    slAgentTrapPort, 1.3
    slDriveFibrePortAAddressingMode, 1.8.1
    slDriveFibrePortALoopId, 1.8.1
    slDriveFibrePortAPortEnabled, 1.8.1
    slDriveFibrePortAPortSpeed, 1.8.1
    slDriveFibrePortAWWN, 1.8.1
    slDriveFibrePortBAdressingMode, 1.8.1
    slDriveFibrePortBLoopId, 1.8.1
    slDriveFibrePortBPortEnabled, 1.8.1
    slDriveFibrePortBPortSpeed, 1.8.1
    slDriveFibrePortBWWN, 1.8.1
    slDriveFibrePortCount, 1.8.1
    slHostInterfaceA1AddressingMode, 1.11
    slHostInterfaceA1LoopId, 1.11
    slHostInterfaceA1PortEnabled, 1.11
    slHostInterfaceA1PortSpeed, 1.11
    slHostInterfaceA2AddressingMode, 1.11
    slHostInterfaceA2LoopId, 1.11
    slHostInterfaceA2PortEnabled, 1.11
    slHostInterfaceA2PortSpeed, 1.11
    slHostInterfaceB1AddressingMode, 1.11
    slHostInterfaceB1LoopId, 1.11
    slHostInterfaceB1PortEnabled, 1.11
    slHostInterfaceB1PortSpeed, 1.11
    slHostInterfaceB2AddressingMode, 1.11
    slHostInterfaceB2LoopId, 1.11
    slHostInterfaceB2PortEnabled, 1.11
    slHostInterfaceB2PortSpeed, 1.11
    SlSNMPPort, 1.17
    SlSNMPTrapPort, 1.17
  power supply, 1.14.1
    redundant, 1.14.1
  PTP variables, 1.13
    slLibLSMConfigMaxPtpAddr, 1.12.2
    slLibLSMConfigMinPtpAddr, 1.12.2

## R

  RE variables
    slAgentHaAlternateIP, 1.3.1
    slAgentHAId, 1.3.1
    slAgentHaSlot, 1.3.1
    slAgentHAState, 1.3.1
    slControllerHaAlternateIp, 1.7
    slControllerHaId, 1.7
    slControllerHaSlot, 1.7
    slControllerHAState, 1.7
  robot, 1.15

## S

  SL150
    accessing SNMP, 2.1
  SL3000
    accessing SNMP, 2.1
  SL500
    accessing SNMP, 2.1
  SL8500
    accessing SNMP, 2.1
  SNMP
    access control, 2.2.4
    community strings support, 2.2.4
    configuration
      process, 2.4
      requirements, 2.2.3
    defined, 2.2
    managing agents, 2.2.3
    port control, 2.2.3
    service information
      configure, 2.9
    settings
      default, 2.3
    supported versions, 2.2.1
    user
      add, 2.6.2
      delete, 2.6.3
      list, 2.6.1, 2.9
      management, 2.6
    v2, 2.2.4
    v3, 2.2.4

## T

  tape, 1.18
  trap
    agent test, 3.3.2
    agent test heartbeat A, 3.3.3
    agent test heartbeat B, 3.3.4
    CAP status check, 3.3.12
    CAP status good, 3.3.10
    CAP status open, 3.3.11
    configuration, 3.2.4
    delete recipient, 2.7.3
    drive status check, 3.3.9
    environment or hardware condition, 3.3.7
    error, 3.2.1
    information, 3.2.3
    library status check, 3.3.6
    library status good, 3.3.5
    numbers, 3.1
    obtaining designation information, 2.5.2
    PTP status check, 3.3.14
    PTP status good, 3.3.13
    recipient
      add, 2.7.2
      delete, 2.7.3
      filtering, 3.1
      list, 2.7.1
      tasks, 2.7
    tape drive status good, 3.3.8
    warning, 3.2.2
  traps
    agent-specific
      definition, 3.3
    event-based
      definition, 3.3
      slAgentTest, 3.3.2
      slAgentTestHeartbeatA, 3.3.3
      slAgentTestHeartbeatB, 3.3.4
      slTrapAgentStart, 3.3.1
      slTrapCapStatusCheck, 3.3.12
      slTrapCapStatusGood, 3.3.10
      slTrapCapStatusOpen, 3.3.11
      slTrapDrvStatusCheck, 3.3.9
      slTrapDrvStatusGood, 3.3.8
      slTrapEnvHdwCheck, 3.3.7
      slTrapLibStatusCheck, 3.3.6
      slTrapLibStatusGood, 3.3.5
      slTrapPtpStatusCheck, 3.3.14
      slTrapPtpStatusGood, 3.3.13
    generated from log entries, 3.2
    generic
      definition, 3.2
      slTrapConfiguration, 3.2.4
      slTrapError, 3.2.1
      slTrapInformation, 3.2.3
      slTrapWarning, 3.2.2

## V

  version variables
    slAgentRevision, 1.3
    slControllerCodeVer, 1.7
    slControllerFirmwareVer, 1.7
    slControllerVersion, 1.7
    slDrivecodeVer, 1.8.1
    slDriveVersion, 1.8.1
    slElevatorCodeVer, 1.9
    slElevatorFirmwareVer, 1.9
    slElevatorVersion, 1.9
    slHostInterfaceCodeVer, 1.11
    slHostInterfaceFirmwareVer, 1.11
    slHostInterfaceVersion, 1.11
    slLibMibVer, 1.12.4
    slLibVersionBootRev, 1.12.10
    slLibVersionFirmDate, 1.12.10
    slLibVersionFirmRev, 1.12.10
    slLibVersionHardware, 1.12.10
    slPtpCodeVer, 1.13
    slPtpFirmwareVer, 1.13
    slPtpVersion, 1.13
    slRobotCodeVer, 1.15
    slRobotFirmwareVer, 1.15
    slRobotVersion, 1.15
    slTrapAsrSuspectFruRevision, 1.19.1
    slTurntableCodeVer, 1.20
    slTurntableFirmwareVer, 1.20
    slTurntableVersion, 1.20