Skip Navigation Links
Exit Print View
| Oracle Solaris Cluster Reference Manual Oracle Solaris Cluster 4.1

Search Scope:

- This Document
- Entire Library

### scconf_transp_adap_bge

- configure the bge transport adapter

## Description

Note - Oracle Solaris Cluster software includes an object-oriented command set. Although Oracle Solaris Cluster software still supports the original command set, Oracle Solaris Cluster procedural documentation uses only the object-oriented command set. For more information about the object-oriented command set, see the `Intro`(1CL) man page.

You can configure `bge` adapters as cluster transport adapters. These adapters can only be used with the `dlpi` transport type. The `bge` adapter is VLAN capable.

The `bge` adapter connects to a transport switch or to another `bge` adapter on a different node. In either case, the connection is made through a transport cable.

When a transport switch is used and the endpoints of the transport cable are configured by using the `scconf` command, the `scinstall` command, or other tools, you are asked to specify a port name on the transport switch. You can provide any port name, or accept the default, as long as the name is unique for the switch.

The default is to set the port name to the node ID hosting the adapter at the other end of the cable.

There are no user configurable properties for cluster transport adapters of this type.

## See Also

`Intro`(1CL), `clinterconnect`(1CL), `clnode`(1CL), `scconf`(1M), `scinstall`(1M), `bge`(7D)

Copyright © 2000, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |