Skip Navigation Links
Exit Print View
| Oracle Solaris Cluster Reference Manual Oracle Solaris Cluster 4.1

Search Scope:

- This Document
- Entire Library

### clconfiguration

- describes the cluster DTD for the Oracle Solaris Cluster configuration XML file

## Description

`clconfiguration` describes the Documentation Type Definition (DTD) for the Oracle Solaris Cluster configuration eXtensible Markup Language (XML) file. The Oracle Solaris Cluster configuration file contains Oracle Solaris Cluster configuration information tagged with XML elements. The file can contain configuration information for one or more clusters, or even for a portion of a cluster. This Oracle Solaris Cluster configuration information can be used for many cluster functions, including cluster configuration backup and cluster duplication.

The DTD defines the elements, their relationships, and their attributes. The element names reflect the content that they provide. For example, the element `<devicegroup>` defines cluster device groups. Elements might have attributes that are used to modify or refine their properties or characteristics. Many of the object-oriented Oracle Solaris Cluster commands include an `export` subcommand that exports cluster object information in the format described in the DTD. Many Oracle Solaris Cluster commands have the option to add, create, and modify Oracle Solaris Cluster objects through the use of cluster configuration XML data.

## Element Hierarchy

The following list provides the element hierarchy required by the DTD. This list uses the following defaults for children and attribute properties:

required

  Unless otherwise specified, one or more is required.

optional

  Unless otherwise specified, there can be zero or one.

    <propertyList>
      <property>
    <state>
    <allNodes>

    <-- Cluster -->

    <cluster>

      <-- Cluster Nodes -->

      <nodelist>
        <node>

      <-- Cluster Transport -->

      <clusterTransport>
        <transportNodeList>
          <transportNode>
            <transportAdapter>
              <transportType>
        <transportSwitchList>
          <transportSwitch>
        <transportCableList>
          <transportCable>
            <endpoint>

      <-- Cluster Global Devices -->

      <deviceList>
        <device>
          <devicePath>

      <-- Cluster Quorum -->

      <clusterQuorum>
        <quorumNodeList>
          <quorumNode>
        <quorumDeviceList>
          <quorumDevice>
            <quorumDevicePathList>
              <quorumDevicePath>

      <-- Cluster Device Groups -->

      <devicegroupList>
        <devicegroup>
          <memberDeviceList>
            <memberDevice>
          <devicegroupNodeList>
            <devicegroupNode>

      <-- Cluster Resource Types -->

      <resourcetypeList>
        <resourcetype>
           <resourcetypeRTRFile>
           <resourcetypeNodeList>
             <resourcetypeNode>
             <methodList>
             <method>
             <parameterList>
               <parameter>

      <-- Cluster Resources -->

      <resourceList>
        <resource>
          <resourceNodeList>
            <resourceNode)
          <monitoredState>

      <-- Cluster Resource Groups -->

      <resourcegroupList>
        <resourcegroup>
          <failoverMode>
          <managedState>
          <resourcegroupNodeList>
            <resourcegroupNode>
          <resourcegroupResourceList>
            <resourcegroupResource>

      <-- Cluster NAS Devices -->

      <nasdeviceList>
        <nasdevice>
           <nasdir>

      <-- Cluster SNMP -->

      <snmpmibList>
        <snmpmib>
      <snmphostList>
        <snmphost>
      <snmpuserList>
        <snmpuser>
      <-- Cluster Telemetrics -->

      <telemetrics>
        <telemetryObjectType>
          <telemetryAttribute>

## ELEMENTS

This section lists and describes all of the elements that are defined in the cluster DTD. If an element has required children or attributes, the required default is one. Optional elements default to zero or one.

`<allNodes>`

  A list of all member nodes in the cluster. The `<allNodes>` element is a generic element.

  The `<allNodes>` element is used to denote all nodes of the cluster.

  Parent:

    `<resourcetypeNodeList>`

  Children:

    None

  Attributes:

    None

`<cluster>`

  The root element of a complete cluster configuration XML file. Every cluster configuration XML file must begin with this element as the root. The DTD can accept only one `<cluster>` element. Subsequent `<cluster>` elements in the cluster configuration XML file are ignored.

  Parent:

    None

  Children:

    Optional:

    - `<propertyList>`

    - `<nodeList>`

    - `<clusterTransport>`

    - `<deviceList>`

    - `<clusterQuorum>`

    - `<deviceGroupList>`

    - `<resourcetypeList>`

    - `<resourcegroupList>`

    - `<resourceList>`

    - `<nasdeviceList>`

    - `<snmpmibList>`

    - `<snmphostList>`

    - `<snmpuserList>`

  Attributes:

    Required:

    - `name`

      The name of the cluster.

`<clusterQuorum>`

  The root element of the cluster quorum configuration. All cluster quorum information is defined in the child elements of the `<clusterQuorum>` element.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<quorumDeviceList>`

    - `<quorumNodeList>`

  Attributes:

    None

`<clusterTransport>`

  The root element of the cluster transport configuration. All cluster transport information is displayed in a sublevel of the `<clusterTransport>` element.

  Parent:

    `<cluster>`.

  Children:

    Optional:

    - `<transportNodeList>`

    - `<transportSwitchList>`

    - `<transportCableList>`

  Attributes:

    None

`<device>`

  A cluster device ID pseudo-driver (DID) device.

  Parent:

    `<deviceList>`

  Children:

    Optional:

    - `<devicePath> (zero or more)`

  Attributes:

    Required:

    - `ctd`

      The UNIX disk name.

    - `name`

      The instance number of the device.

`<devicegroup>`

  The root element of a cluster device-group instance. All aspects of an individual device group are defined in the child elements of the `<devicegroup>` element.

  Parent:

    `<devicegroupList>`

  Children:

    Optional:

    - `<devicegroupNodeList>`

    - `<memberDeviceList>`

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      The name of the device group. The `name` attribute can be any valid sequence of characters.

    - `type`

      The type of the device group. The `type` attribute can have a value of `rawdisk`, `vxvm`, `svm`, or `sds`.

`<devicegroupList>`

  A list of all the cluster device groups.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<devicegroup>`

      One `<devicegroup>` element can be used for each device group in the cluster.

  Attributes:

    None

`<devicegroupNode>`

  The node on which a device group is located.

  Parent:

    `<devicegroupNodeList>`

  Children:

    None

  Attributes:

    Required:

    - `nodeRef`

      Specifies the name of a cluster node.

`<devicegroupNodeList>`

  A list of nodes on which a device group is located.

  Parent:

    `<devicegroup>` (1 or more)

  Children:

    Required:

    - `<devicegroupNode> (1 or more)`

  Attributes:

    None

`<deviceList>`

  A list of cluster DID devices.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<device>`

  Attributes:

    Fixed:

    - `readonly`

      The `readonly` attribute has a fixed value of `true`.

`<deviceNode>`

  The node and disk device on which a particular `<device>` exists.

  Parent:

    `<device>`

  Children:

    None

  Attributes:

    Required:

    - `nodeRef`

      The name of the node on which an instance exists.

`<endpoint>`

  One of the transport endpoints.

  Parent:

    `<transportCable>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The name of the adapter or switch.

    - `nodeRef`

      The name of the node that hosts the specified adapter. The `nodeRef` attribute is required only if the `type` attribute is set to `adapter`.

    - `type`

      The `type` attribute can be set to either `adapter` or `switch`.

      If the `type` attribute is set to `adapter`, you must specify a `nodeRef` attribute.

      If the `type` attribute is set to `switch`, you can specify a `port` attribute. However, the `port` attribute is not required.

    Optional:

    - `port`

      The number of the port on the switch. Specify the `port` attribute only if the `type` attribute is set to `switch`.

`<failoverMode>`

  The failover mode of a resource group.

  Parent:

    `<resourcegroup>`

  Children:

    None

  Attributes:

    Required:

    - `value`

      The `value` attribute can be set to `failover` or `scalable`.

`<managedState>`

  Indicates whether a resource group is managed or unmanaged.

  Parent:

    `<resourcegroup>`

  Children:

    None

  Attributes:

    Required:

    - `value`

      The `value` attribute can be either `true` or `false`.

`<memberDevice>`

  The member name of a particular device group. If the `<devicegroup>` is a set of type `rawdisk`, then you must specify one or more `<member>` elements, each with the name of the raw-disk path.

  Parent:

    `<memberDeviceList>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The name of the member.

`<memberDeviceList>`

  A list of device group members.

  Parent:

    `<devicegroup>` (one or more)

  Children:

    Required:

    - `<memberDevice>`

  Attributes:

    None

`<method>`

  Mapping between a generic method type and the actual method name for a specific resource type.

  Parent:

    `<methodList>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The actual name of the method for the resource type.

    - `type`

      The type of method for the resource type. You can specify the following types:

      - `MONITOR_CHECK`

      - `MONITOR_START`

      - `MONITOR_STOP`

      - `PRENET_START`

      - `START`

      - `STOP`

      - `VALIDATE`

      - `UPDATE`

`<methodList>`

  A list of all of the `<method>` elements that are available for a specific `<resourcetype>`.

  Parent:

    `<resourcetype>`

  Children:

    Optional:

    - `<method>`

  Attributes:

    Fixed:

    - `readonly`

      The `readonly` attribute has a fixed value of `true`.

`<monitoredState>`

  A Boolean value that indicates a portion of an element's state in the cluster. For example, the `<monitoredState>` of a resource specifies whether the resource is monitored, but does not specify whether the resource is available.

  Parent:

    `<resource>`

  Children:

    None

  Attributes:

    Required:

    - `value`

      The `value` attribute can be set to `true` or `false`.

`<nasdevice>`

  A single instance of a NAS device on the cluster.

  Parent:

    `<nasdeviceList>`

  Children:

    Optional:

    - `<nasdir>`

  Attributes:

    Required:

    - `name`

      The hostname of the NAS device.

    - `type`

      The type of NAS device. You must specify `sun_uss` for a Sun ZFS Storage Appliance.

    Optional:

    - `userid`

      The user name that is required to access the NAS device.

`<nasdeviceList>`

  A list of all NAS devices on the cluster.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<nasdevice>`

  Attributes:

    None

`<nasdir>`

  One directory on a NAS device. Each NAS device can have multiple NAS directories.

  Parent:

    `<nasdevice>`

  Children:

    None

  Attributes:

    Required:

    - `path`

      The path to the NAS directory.

`<node>`

  A cluster node. Specify one `<node>` element for each node in the cluster.

  Parent:

    `<nodeList>`

  Children:

    Optional:

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      Must be equal to the name of the node.

    Optional:

    - `id`

      The cluster node ID. If not specified, the cluster node ID attribute is provided a default value of an empty string.

`<nodeList>`

  A list of all nodes in the cluster.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<node>`

      At least one `node` attribute must be supplied for each node on the cluster.

  Attributes:

    None

`<parameter>`

  A set of attributes that describes the `<method>` element timeout values and other parameters for a cluster resource type.

  Parent:

    `<parameterList>`

  Children:

    None

  Attributes:

    Required:

    - `extension`

      The `extension` attribute can be set to `true` or `false`.

    - `name`

      The name of the parameter.

    - `tunability`

      The value of the parameter's tunability. The `tunability` attribute can be set to one of the following values: `atCreation`, `anyTime`, or `whenDisabled`.

    - `type`

      The type of the parameter. The `type` attribute can be set to one of the following values: `boolean`, `enum`, `int` , `string`, or `stringArray`.

    Optional:

    - `default`

      The default value of this parameter if a value is not explicitly specified. For example, the default for the `method` element timeout is `START`.

    - `description`

      A description of the parameter. If not defined, this attribute defaults to an empty string.

    - `enumList`

      An enumerated list of objects. For example, the attribute might be a list of failover modes in order of preference.

    - `maxLength`

      The maximum length of a `string` or `stringArray` type parameter.

    - `minArrayLength`

      The minimum size of an `stringArray` type parameter.

    - `minLength`

      The minimum length of a `string` or `stringArray` type parameter.

`<parameterList>`

  A list of `<parameter>` elements that describes a resource type.

  Parent:

    `<resourcetype>`

  Children:

    Optional:

    - `<parameter>`

  Attributes:

    Fixed:

    - `readonly`

      The `readonly` attribute has a fixed value of `true`.

`<property>`

  A generic element that describes one property. The property is not specific to any subset of cluster related configuration.

  Parent:

    `<propertyList>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The name of the property.

    - `value`

      The value of the property.

    Optional:

    - `readonly`

      The `readonly` attribute can be set to `true` or `false`. If this value is not specified, the attribute defaults to the value `false`.

    - type

      The property type.

`<propertyList>`

  A list of `<property>` elements. The `<propertyList>` element is a generic element.

  Parents:

    `<cluster>`, `<deviceGroup>`, `<node>`, `<quorumDevice>`, `<quorumNode>`, `<resource>`, `<resourceNode>`, `<resourcegroup>`, `<resourceType>`, `<transportAdapter>`, `<transportType>`

  Children:

    `Optional:`

    - `<property>`

  Attributes:

    Optional:

    - `extension`

      This attribute can have one of the following values: `true`, `false`, `mixed`, or `doesNotApply`. If a value is not specified, the `extension` attribute has a default value of `doesNotApply`.

    - `readonly`

      This attribute can have a value of `true` or `false`. If a value is not specified, the `readonly` attribute has a default value of `false`.

`<quorumDevice>`

  An individual cluster quorum device.

  Parent:

    `<quorumDeviceList>`

  Children:

    Optional:

    - `<propertyList>`

      The `<quorumDevice>` element can have only one `<propertyList>` child.

    - `<quorumDevicePathList>`

      The `<quorumDevice>` element can have only one `<quorumDevicePathList>` child.

  Attributes:

    Required:

    - `name`

      The name of the quorum device.

    - `type`

      The type of quorum device that is referenced by this element. The `type` attribute can be set to `scsi` or `quorum_server`.

`<quorumDeviceList>`

  A list of all quorum devices in the cluster.

  Parent:

    `<clusterQuorum>`

  Children:

    Optional:

    - `<quorumDevice>`

  Attributes:

    None

`<quorumDevicePath>`

  The path to a cluster quorum device.

  Parent:

    `<quorumDevicePathList>`

  Children:

    Optional:

    - `<state>`

      The `<quorumDevicePath>` element can have only one `<state>` child.

  Attributes:

    Required:

    - `nodeRef`

      The name of the node that the quorum device resides on.

`<quorumDevicePathList>`

  A list of all paths to a particular `<quorumDevice>`.

  Parent:

    `<quorumDevice>`

  Children:

    Required:

    - `<quorumDevicePath>`

  Attributes:

    Fixed:

    - `readonly`

      The `readonly` attribute is set to `true`.

`<quorumNode>`

  A node in the cluster that participates in the cluster quorum.

  Parent:

    `<quorumNodeList>`

  Children:

    Optional:

    - `<propertyList>`

  Attributes:

    Required:

    - `<nodeRef>`

      The name of the node.

`<quorumNodeList>`

  A list of all nodes that participate in the cluster quorum. In a functional cluster that is not in `installmode`, this list typically contains all nodes in the cluster. In a cluster that is still in `installmode`, this list might contain only one of the cluster nodes.

  Parent:

    `<clusterQuorum>`

  Children:

    Required:

    - `<quorumNode>`

  Attributes:

    Fixed:

    - `readonly`

      The `readonly` attribute is set to `true`.

`<resource>`

  A cluster resource.

  Parent:

    `<resourceList>`

  Children:

    Optional:

    - `<resourceNodeList>`

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      The name of the resource.

    - `resourcegroupRef`

      The resource group to which the resource belongs.

    - `resourcetypeRef`

      The type of resource that is described by this element.

`<resourceList>`

  A list of the root node for the cluster resources that are defined in the configuration.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<resource>`

  Attributes:

    None

`<resourcegroup>`

  A cluster resource group.

  Parent:

    `<resourcegroupList>`

  Children:

    Required:

    - `<failoverMode>`

    - `<managedState>`

    - `<resourcegroupNodeList>`

    - `<resourcegroupResourceList>`

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      The name of the resource.

`<resourcegroupList>`

  The root node for the cluster resource groups that are defined in the configuration.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<resourcegroup>`

  Attributes:

    None

`<resourcegroupNode>`

  The node on which a resource group is defined.

  Parent:

    `<resourcegroupNodeList>`

  Children:

    None

  Attributes:

    Required:

    - `nodeRef`

      The name of the cluster node.

`<resourcegroupNodeList>`

  The cluster nodes on which a particular resource group operates.

  Parent:

    `<resourcegroup>`

  Children:

    Required:

    - `<resourcegroupNode>`

  Attributes:

    None

`<resourcegroupResource>`

  A cluster resource that belongs to a particular resource group.

  Parent:

    `<resourcegroupResourceList>`

  Children:

    None

  Attributes:

    Required:

    - `resourceRef`

      The name of the resource.

`<resourcegroupResourceList>`

  A list of the resources that are defined in a resource group.

  Parent:

    `<resourcegroup>`

  Children:

    Optional:

    - `<resourcegroupResource>`

  Attributes:

    None

`<resourceNode>`

  The node on which a resource is defined.

  Parent:

    `<resourceNodeList>`

  Children:

    Required:

    - `<state>`

    - `<monitoredState>`

    Optional:

    - `<propertyList>`

  Attributes:

    Required:

    - `nodeRef`

      The name of the resource type.

`<resourcetype>`

  A cluster resource type that is available in the cluster.

  Parent:

    `<resourcetypeList>`

  Children:

    Optional:

    - `<resourcetypeRTRFile>`

    - `<resourcetypeNodeList>`

    - `<methodList>`

    - `<parameterList>`

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      The name of the resource type.

`<resourcetypeList>`

  The root node of the cluster resource types that are defined in the configuration.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<resourcetype>`

  Attributes:

    None

`<resourcetypeNode>`

  A node on which a resource type is defined.

  Parent:

    `<resourcetypeNodeList>`

  Children:

    None

  Attributes:

    Required:

    - `nodeRef`

      The name of the cluster node.

`<resourcetypeNodeList>`

  A list of the cluster nodes on which a particular resource type exists.

  Parent:

    `<resourcetype>`

  Children:

    Required : The `<resourcetypeNodeList>` element must contain either one or more `<resourcetypeNode>` elements or exactly one `<allNodes>` element.

    - `<resourcetypeNode>`

    - `<allNodes>`

  Attributes:

    None

`<resourcetypeRTRFile>`

  The name of a resource type registration (RTR) file that describes a particular resource type.

  Parent:

    `<resourcetype>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The name of the RTR file.

`<snmphost>`

  The SNMP host and community that are configured on a cluster node.

  Parent:

    `<snmphostList>`

  Children:

    None

  Attributes:

    Required:

    - `community`

      The SNMP community name.

    - `name`

      The name of the instance.

    - `nodeRef`

      The node on which the SNMP host and community exist.

`<snmphostList>`

  A list of the SNMP hosts and communities that are configured on a cluster node.

  Parent:

    `cluster>`

  Children:

    Optional:

    - `<snmphost>`

  Attributes:

    None

`<snmpmib>`

  An SNMP MIB that is on a cluster node.

  Parent:

    `<snmpmibList>`

  Children:

    Optional:

    - `state`

  Attributes:

    Required:

    - `name`

      The name of the MIB.

    - `nodeRef`

      The node on which the SNMP MIB exists.

    Optional:

    - `protocol`

      The SNMP protocol that the MIB will use. This attribute defaults to `SNMPv2`.

    - `value`

      SNMPv3 or SNMPv2

`snmpmibList`

  A list of the SNMP MIBs that are on a cluster node.

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<snmpmib>`

  Attributes:

    None

`<snmpuser>`

  The SNMPv3 user that is configured on a cluster node.

  Parent:

    `<snmpuserList>`

  Children:

    None

  Attributes:

    Required:

    - `name`

      The name of the user.

    - `nodeRef`

      The node on which the SNMPv3 user exists.

    - `auth`

      The `auth` attribute can be set to `MD5` or `SHA`.

    Optional:

    - `defaultUser`

      The `defaultUser` attribute can be set to `yes` or `no`. If a value is not specified, the attribute defaults to whichever value is appropriate, based on the node configuration.

    - `defaultSecurityLevel`

      The security level of the user. The `security` attribute can be set to one of the following values:

      - `authPriv`

      - `authNoPriv`

      - `noAuthNoPriv`

`<snmpuserList>`

  A list of the SNMPv3 users that are configured on a cluster node.

  Parent:

    `<cluster>`

  Children:

    `<snmpuser>`

  Attributes:

    None

`<state>`

  The state of various objects within the cluster configuration. The `<state>` element is a generic element.

  Parent:

    `<quorumDevicePath>`, `<resourceNode>`, `snmpmib>`, `telemetryAttribute`, `<transportAdapter>`, `<transportCable>`, `<transportSwitch>`

  Children:

    None

  Attributes:

    Required:

    - `value`

      The `value` attribute can be set to `enabled` or `disabled`.

`<telemetrics>`

  Cluster monitoring thresholds

  Parent:

    `<cluster>`

  Children:

    Optional:

    - `<telemetryObjectType>`

  Attributes:

    None

`<telemetryAttribute>`

  The attributes of system resources that you can monitor.

  Parent:

    `<telemetryObjectType>`

  Children:

    Required:

    - `<state>` (1 or more)

  Attributes:

    Required:

    - `name`

      The name of the attribute.

`<telemetryObjectType>`

  The types of objects you can monitor.

  Parent:

    `<telemetrics>`

  Children:

    Required:

    - `<telemetryAttibute>`

  Attributes:

    Required:

    - name

      The name of the attribute.

`<transportAdapter>`

  A network adapter that is used in the private cluster transport.

  Parent:

    `<transportNode>`

  Children:

    Optional:

    - `<state>`

    - `<transportType>`

    - `<propertyList>`

  Attributes:

    Required:

    - `name`

      The name of the network adapter.

`<transportCable>`

  A network cable that is used in the private cluster transport. The cable does not necessarily imply a physical cable, but rather a path between two `<endpoint>` elements.

  Parent:

    `<transportCableList>`

  Children:

    Required:

    - `<endpoint>`

      The `<transportCable>` element must have two `<endpoint>` elements. Each `endpoint` element must describe one of the cable endpoints.

    Optional:

    - `<state>`

      The `<transportCable>` element can have one `<state>` element.

  Attributes:

    None

`<transportCableList>`

  A list of the network cables that are used to connect two cluster `<endpoint>` elements.

  Parent:

    `<clusterTransport>`

  Children:

    `Optional:`

    - `<transportCable>`

  Attributes:

    None

`<transportNode>`

  One of the cluster nodes that is used in the private cluster transport. Specify one `<transportNode>` element for each node of the cluster.

  Parent:

    `<transportNodeList>`

  Children:

    Optional:

    - `<nodeRef>`

  Attributes:

    Required:

    - `transportAdapterList`

      The name of the cluster node.

`<transportNodeList>`

  A list of the nodes that are used in the private cluster transport. This list of nodes always contains the same set of nodes as the members of the cluster.

  Parent:

    `<clusterTransport>`

  Children:

    Optional:

    - `<transportNode>`

  Attributes:

    None

`<transportSwitch>`

  A cluster transport switch.

  Parent:

    `<transportSwitchList>`

  Children:

    Optional:

    - `<state>`

  Attributes:

    Required:

    - `name`

      The name of the transport switch.

    Optional:

    - `port`

      The number of the port on the switch.

`<transportSwitchList>`

  A list of the network switches that are used by the private cluster transport system.

  Parent:

    `<clusterTransport>`

  Children:

    Optional:

    - `<transportSwitch>`

  Attributes:

    None

`<transportType>`

  The type of network transport that is used for a `<transportAdapter>` element.

  Parent:

    `<transportAdapter>`

  Children:

    Optional:

    - `<propertyList>`

  Attributes:

    Required:

    - `value`

      The `value` attribute can be set to `dlpi` or `rsm`.

## Files

`/usr/cluster/lib/xml/cluster.dtd`

  The document type definition (DTD) file that defines the structure of the Oracle Solaris Cluster configuration XML file.

## See Also

`Intro`(1CL), `cluster`(1CL)

http://www.w3.org/XML/

Copyright © 2000, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |