Skip Headers

StorageTek SL150 Modular Tape Library System Systems Assurance Guide E22579-02 |
| Library | Contents

Previous |

# Index

A B C D E F I L M N O P R S T W

## A

  addressing, USER physical, A.2
  air quality, C.2

## B

  bridged drive, B.1.1
  bridging interface, 1

## C

  cables
    Ethernet, 3.2.1
    Fibre Channel
      multimode, 3.2.2
      plenum, 3.2.2
      riser, 3.2.2
    SAS, 3.2.3
  cartridge magazine
    description, 1
    part number, 3.1
  cartridges
    locations
      diagnostic & cleaning, A.2.3
    placement in slots, A.1
  class 1 laser product, 1.4
  cleaning procedures, data center, C.9
  command
    SCSI MOVE, B.1.3
    SCSI READ ELEMENT STATUS, B.1.3
  contaminants, controlling, C
  control interface, 1

## D

  data center cleaning procedures, C.9
  description, SL150, 1
  drive, tape, 1, 1.10

## E

  environmental
    contaminants, C.1
    information, SL150, 1.9
  Ethernet cables, 3.2.1

## F

  Fibre Channel cables, 3.2.2
  filtration, C.7

## I

  interface cables, 3.2.2, 3.2.3
  interface, library control, 1

## L

  labels, ordering, 3.4
  laser product, 1.4
  Left side wall, A.1
  library control interface, 1
  locations
    diagnostic & cleaning cartridges, A.2.3
    tape slots, A.2

## M

  magazine
    cartridge, 1
    part number, 3.1
  mailslot, 1.5
    shared, B.1.3
    slots, B
  media
    ordering, 3.4
    types supported, 1.10
  multimode cable part numbers, 3.2.2

## N

  numbering
    cartridges
      diagnostic & cleaning cartridges, A.2.3
    SCSI element, B.1.1, B.1.1
    tape slots, A.2

## O

  ordering SL150, 3

## P

  part numbers
    Ethernet cables, 3.2.1
    fiber optic cables, 3.2.2
    power cords, 3.3
    SAS cables, 3.2.3
    SL150, 3.1
  partition
    description, 1.7
    feature, B.1.1
    mailslot assignment, B.1.3
    setting of, B.1
  placement, data cartridges into slots, A.1
  plenum cables, 3.2.2
  power cord part numbers, 3.3

## R

  Right side wall, A.1
  riser cables, 3.2.2

## S

  SAS
    cable part number, 3.2.3
    serial connection, 2.4
  SCSI MOVE command, B.1.3
  SCSI READ ELEMENT STATUS command, B.1.3
  service clearance, 2.5
  shared mailslot, B.1.3
  SL150
    description, 1
    mailslot, 1.5
    ordering, 3
    part numbers, 3.1
    partitions, 1.7
    tape drive, 1, 1.10
  slots
    diagnostic & cleaning cartridges, A.2.3
    overview, A

## T

  tape cartridge
    ordering, 3.4
    types supported, 1.10
  tape drive, 1, 1.10

## W

  wall
    Left side, A.1
    Right side, A.1
  Windows device driver, 2.2